{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["清单"],"not_rendered":{"comments":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"清单","index":0,"n_rows":20,"n_cols":7,"rows_kept":20,"merged":[[0,0,0,6],[19,0,19,1]],"flags":["formulas_cached_only"]}
["华光学院新校区宿舍楼监控系统设备清单"]
["序号","名称","产品型号","规 格 型 号","单位","数量","备 注"]
[1,"网络硬盘录像机",null,"支持32路720P/16路1080P输入和解码/100Mbps RJ45接口，直连IPC/1路VGA输出，1路HDMI输出100/1000M 自适应,RJ45接口/2个USB 2.0接口、4个SATAII硬盘","台",3]
[2,"硬盘",null,"监控专用4T/7200转","块",3]
[3,"IP枪机",null,"1080P高清网络摄像机/双灯/200万像素/H.264编码/红外距离50米","个",23]
[4,"IP半球",null,"1080P高清网络摄像机/单灯/200万像素/H.264编码/红外距离30米","个",30]
[5,"支架",null,"摄像机支架","个",23]
[6,"电源",null,"直流电源2A/12V","个",53]
[7,"交换机",null,"8口100M/1000M","台",2]
[8,"交换机",null,"24口100M/1000M","台",3]
[9,"光纤收发器",null,"100M/1000M","对",3]
[10,"KVM切换器",null,"USB8口切换器/配线","套",1]
[11,"机柜",null,"24U/标准网络机柜","台",1]
[12,"网线","国标",null,"箱",9]
[13,"电源线","国标",null,"米",2080]
[14,"线管","国标",null,"米",420]
[15,"线管","国标",null,"米",210]
[16,"辅助材料","国标","PVC弯头，BNC头，管卡，软管等","项",1]
[17,"人工费",null,"布线及设备安装调试费","点",53]
["合计"]